LuSiD’s Arcade Flashback 
Cabinet Plans 
Revision 7 

I.  Assembly Notes 
  
It’s a lot easier to cut the cut the groove for the T molding  before assembling the cabinet.  
The 26” edges of the cabinet bottom  need T molding, as well as the cabinet sides. 
 
A few edges should be cut at a 45° angle for everything to fit together.  These are both 
26” edges of the  Cabinet Back – Angled section, and one  30” edge of the Control panel 
box Back. 
 
All the measurements assume that 5/8” wood is used for the cabinet.  If  3/4" wood is 
used, the Coin Door should be 26” X 29 ¾”, and the CP Box Sides should be 14 ½”  deep. 
 
To change the width of the cabinet to accommodate a wider or narrower monitor or TV, 
change all the 26” measurements to the desired width. 
 
II. Assembly Sequence 
  1.  Start by assembling the cabinet bottom.   
The kick plates and lower supports create a  
support frame for the base of the cabinet.   
You’ll end up with something like this: 

 Bottom View 
2.  Next turn it over, frame side down, and attach the side panels.  With 6 –8 screws 
on each side it should hold itself together long enough to attach the top, back and 
sides, which should all be recessed about ½” from the edge of the side panels. 

3.  Assemble the control panel box seperately, and then attach  
it to the cabinet.  The bottom of the CP box fits inside the  
square created by the 4 sides.  The Control Panel  top is  
held on with velcro. 
Side view of CP-Box. Front, back & 
bottom 

4.  Cut the hole for you coin door (if you plan on using one) and attach the T molding 
to the cabinet before mounting the door on  its hinges.  Otherwise the T molding 
may affect the alignment of the hinges 
LuSiD’s Arcade Flashback, Cabinet Design, rev. 7, page 1 

  

 

 

Monitor Shelf 
(26” X 22”) 
Control 
Panel 
Cabinet Side 1 
      = 1 inch 
 
LuSiD’s Arcade Flashback , Cabinet  Design, rev. 7, page 2 

  

 

 
 
 Control Panel Box -Bottom  
 
 (30” X 13”) 
 
Control Panel Box - Back – (30” X 5 ½”) 
Control Panel Box  – Front - (30” X 3 ½”) 
Control 
Panel 
 Cabinet Side 2 
       = 1 inch 
 
LuSiD’s Arcade Flashback , Cabinet  Design, rev. 7, page 3 

  

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

Cabinet Bottom 
( 26” X 38” ) 

 

Cabinet Back 
Speaker Panel 
Angled section 
(below the marquee) 
(26” X 22”) 
( 26” X 24” ) 

 

 

 
Cabinet Back 
Cabinet Front 
Top section 
Coin Door 
( 26” X 18” ) 
( 26” X 30” ) 

  
Cabinet Back 
Bottom section 
( 26” X 18” ) 
CP box – Side 1 

 
 
CP Box – Side 2 
----------- 14 ¼ “ -------------
- 
       = 1 inch 
 
LuSiD’s Arcade Flashback , Cabinet  Design, rev. 7, page 4 
 
�2礼�